//Verison=2.2
//Example,Don't Delete flowing text!
//Button NIMI // Generator NIMI 
//Button NIMI 100 // Generator NIMI and Delay 100ms, 100 not is nessary
//Button INT0 // Generator INT0 and Delay 200ms
//Button RESETAMBE3000
//Button RESET3252
//Send 1 command, Receive 2 response with one is not verify.
//Command ID: CARRIER_LOST // necessary!
//Summary  // not essential, 
//Send command: 61 00 02 00 19 00 // necessary!
//Pause=300 // not essential, unit: ms; Pause 300ms after Send command
//Timeout=100 // not essential, unit: ms; if not receive '84 A9 61 ...' in 100ms after send command, Timeout error will happen!
//*Receive Data: 61 00 02 51 19 00 // not essential, receive but not verify
//Receive Data: 61 00 02 51 19 20 // not essential, receive and verify 
//.Set x = AA B0  -- Define var x ; Added in ver2.2
// ... 61 00 02 00 19 {x}   --- use the defined var, The {x} will be replaced with AA B0 
//
.Set READY_VAR = 01
Command ID:	DPMR_CC
Send	Command: 84 A9 61 00 04 03 5C 77 F5 D5
Receive	Command:84 A9 61 00 02 03 5C 00
Command ID: WORK_MODE_DUPLEX
Send command: 84 A9 61 00 04 00 18 03 00 00
Receive Data: 84 A9 61 00 02 00 18 00
Command ID: PROCESS_MODE
Send command: 84 A9 61 00 02 00 1A 03
Receive Data: 84 A9 61 00 02 00 1A 00
Command ID:	ADDRESSING_MODE
Send	Command: 84 A9 61 00 02 03 28 01
Receive	Command:84 A9 61 00 02 03 28 00
Command ID:	REPORT_FIELD
Send	Command: 84 A9 61 00 02 00 1D 7f
Receive	Command:84 A9 61 00 02 00 1D 00

Command ID: PROTOCOL_OPTION  
Send command: 84 A9 61 00 02 00 55 80  //old all call
Receive Data: 84 A9 61 00 02 00 55 00

Command ID: DPMR_HT_CI
Send command: 84 A9 61 00 03 03 57 00 00
Receive Data: 84 A9 61 00 02 03 57 00

Command ID: DPMR_CALLED_ID
Send command: 84 A9 61 00 05 03 52 12 34 56 70
Receive Data: 84 A9 61 00 02 03 52 00

Command ID: DPMR_OWN_ID
Send command: 84 A9 61 00 05 03 53 12 34 56 70
Receive Data: 84 A9 61 00 02 03 53 00

Command ID: CARRIER_LOST
Send command: 84 A9 61 00 02 00 19 00
Receive Data: 84 A9 61 00 02 00 19 00
Pause 500
Command ID: CARRIER_READY
Send command: 84 A9 61 00 02 00 19 {READY_VAR}
Receive Data: 84 A9 61 00 02 00 19 00

//FOR DPMR VOICE CALL
Command ID:	CALL_START
Send	Command: 84 A9 61 00 02 00 20 02
Receive	Command:84 A9 61 00 02 00 20 00
PAUSE 50
Receive	Data:84 A9 61 00 03 30 57 00 00
Receive	Data:84 A9 61 00 02 30 54 02
Receive	Data:84 A9 61 00 04 30 50 1B 91 FD
Receive	Data:84 A9 61 00 04 30 51 1B 91 FD
Receive	Data:84 A9 61 00 05 30 52 12 34 56 70
Receive	Data:84 A9 61 00 05 30 53 12 34 56 70
Receive	Data:84 A9 61 00 04 30 5C 77 F5 D5
Receive	Data:84 A9 61 00 02 30 27 00


Command ID:	CALL_END
Send	Command: 84 A9 61 00 01 00 21 00
Receive	Data:84 A9 61 00 02 00 21 00
Receive	Data:84 A9 61 00 02 20 17 0A
Receive	Data:84 A9 61 00 04 30 4B 00 00 00
Pause 500
Command ID: DPMR_CALLED_ID
Send command: 84 A9 61 00 05 03 52 1A AA AA A0
Receive Data: 84 A9 61 00 02 03 52 00

Command ID: CARRIER_LOST
Send command: 84 A9 61 00 02 00 19 00
Receive Data: 84 A9 61 00 02 00 19 00
Pause 500
Command ID: CARRIER_READY
Send command: 84 A9 61 00 02 00 19 {READY_VAR}
Receive Data: 84 A9 61 00 02 00 19 00


Command ID:	CALL_START
Send	Command: 84 A9 61 00 02 00 20 02
Receive	Command:84 A9 61 00 02 00 20 00
PAUSE 50
Receive	Data:84 A9 61 00 03 30 57 00 00
Receive	Data:84 A9 61 00 02 30 54 02
Receive	Data:84 A9 61 00 04 30 50 2F 23 62   //****************************
Receive	Data:84 A9 61 00 04 30 51 1B 91 FD
Receive	Data:84 A9 61 00 05 30 52 1A AA AA A0
Receive	Data:84 A9 61 00 05 30 53 12 34 56 70
Receive	Data:84 A9 61 00 04 30 5C 77 F5 D5
Receive	Data:84 A9 61 00 02 30 27 02

Command ID:	CALL_END
Send	Command: 84 A9 61 00 01 00 21 00
Receive	Data:84 A9 61 00 02 00 21 00
Receive	Data:84 A9 61 00 02 20 17 0A
Receive	Data:84 A9 61 00 04 30 4B 00 00 00
Pause 500

////////////////////////

Command ID: DPMR_CALLED_ID
Send command: 84 A9 61 00 04 03 50 18 CC 3E     //BCD:0A AA AA A0
Receive Data: 84 A9 61 00 02 03 50 00

Command ID: DPMR_OWN_ID
Send command: 84 A9 61 00 05 03 53 46 32 45 60
Receive Data: 84 A9 61 00 02 03 53 00

Command ID: CARRIER_LOST
Send command: 84 A9 61 00 02 00 19 00
Receive Data: 84 A9 61 00 02 00 19 00
Pause 500
Command ID: CARRIER_READY
Send command: 84 A9 61 00 02 00 19 {READY_VAR}
Receive Data: 84 A9 61 00 02 00 19 00


Command ID:	CALL_START
Send	Command: 84 A9 61 00 02 00 20 02
Receive	Command:84 A9 61 00 02 00 20 00
PAUSE 50
Receive	Data:84 A9 61 00 03 30 57 00 00
Receive	Data:84 A9 61 00 02 30 54 02
Receive	Data:84 A9 61 00 04 30 50 18 CC 3E
Receive	Data:84 A9 61 00 04 30 51 67 7C 26
Receive	Data:84 A9 61 00 05 30 52 0A AA AA A0
Receive	Data:84 A9 61 00 05 30 53 46 32 45 60
Receive	Data:84 A9 61 00 04 30 5C 77 F5 D5
Receive	Data:84 A9 61 00 02 30 27 05

Command ID:	CALL_END
Send	Command: 84 A9 61 00 01 00 21 00
Receive	Data:84 A9 61 00 02 00 21 00
Receive	Data:84 A9 61 00 02 20 17 0A
Receive	Data:84 A9 61 00 04 30 4B 00 00 00
Pause 1000

Command ID: DPMR_CALLED_ID
Send command: 84 A9 61 00 04 03 50 F8 33 A6     //BCD:AA AA AA A0
Receive Data: 84 A9 61 00 02 03 50 00

Command ID: DPMR_OWN_ID
Send command: 84 A9 61 00 05 03 53 06 33 88 90
Receive Data: 84 A9 61 00 02 03 53 00

Command ID: CARRIER_LOST
Send command: 84 A9 61 00 02 00 19 00
Receive Data: 84 A9 61 00 02 00 19 00
Pause 500
Command ID: CARRIER_READY
Send command: 84 A9 61 00 02 00 19 {READY_VAR}
Receive Data: 84 A9 61 00 02 00 19 00


Command ID:	CALL_START
Send	Command: 84 A9 61 00 02 00 20 02
Receive	Command:84 A9 61 00 02 00 20 00
PAUSE 50
Receive	Data:84 A9 61 00 03 30 57 00 00
Receive	Data:84 A9 61 00 02 30 54 02
Receive	Data:84 A9 61 00 04 30 50 F8 33 A6
Receive	Data:84 A9 61 00 04 30 51 0E 26 D1
Receive	Data:84 A9 61 00 05 30 52 AA AA AA A0
Receive	Data:84 A9 61 00 05 30 53 06 33 88 90
Receive	Data:84 A9 61 00 04 30 5C 77 F5 D5
Receive	Data:84 A9 61 00 02 30 27 02

Command ID:	CALL_END
Send	Command: 84 A9 61 00 01 00 21 00
Receive	Data:84 A9 61 00 02 00 21 00
Receive	Data:84 A9 61 00 02 20 17 0A
Receive	Data:84 A9 61 00 04 30 4B 00 00 00
Pause 1000


///////////////////////


Command ID: PROTOCOL_OPTION  
Send command: 84 A9 61 00 02 00 55 88  //Interim all call**************************************************************
Receive Data: 84 A9 61 00 02 00 55 00


Command ID: DPMR_CALLED_ID
Send command: 84 A9 61 00 04 03 50 FF FD FD //bcd:9A AA AA A0
Receive Data: 84 A9 61 00 02 03 50 00

Command ID: DPMR_OWN_ID
Send command: 84 A9 61 00 05 03 53 92 34 56 70
Receive Data: 84 A9 61 00 02 03 53 00

Command ID: CARRIER_LOST
Send command: 84 A9 61 00 02 00 19 00
Receive Data: 84 A9 61 00 02 00 19 00
Pause 500
Command ID: CARRIER_READY
Send command: 84 A9 61 00 02 00 19 {READY_VAR}
Receive Data: 84 A9 61 00 02 00 19 00


Command ID:	CALL_START
Send	Command: 84 A9 61 00 02 00 20 02
Receive	Command:84 A9 61 00 02 00 20 00
PAUSE 50
Receive	Data:84 A9 61 00 03 30 57 00 00
Receive	Data:84 A9 61 00 02 30 54 02
Receive	Data:84 A9 61 00 04 30 50 FF FD FD
Receive	Data:84 A9 61 00 04 30 51 CE 4B 1D
Receive	Data:84 A9 61 00 05 30 52 9A AA AA A0
Receive	Data:84 A9 61 00 05 30 53 92 34 56 70
Receive	Data:84 A9 61 00 04 30 5C 77 F5 D5
Receive	Data:84 A9 61 00 02 30 27 02

Command ID:	CALL_END
Send	Command: 84 A9 61 00 01 00 21 00
Receive	Data:84 A9 61 00 02 00 21 00
Receive	Data:84 A9 61 00 02 20 17 0A
Receive	Data:84 A9 61 00 04 30 4B 00 00 00
Pause 500

Command ID: DPMR_CALLED_ID
Send command: 84 A9 61 00 04 03 50 FF FD FC //bcd:8A AA AA A0
Receive Data: 84 A9 61 00 02 03 50 00

Command ID: DPMR_OWN_ID
Send command: 84 A9 61 00 05 03 53 82 32 45 60
Receive Data: 84 A9 61 00 02 03 53 00

Command ID: CARRIER_LOST
Send command: 84 A9 61 00 02 00 19 00
Receive Data: 84 A9 61 00 02 00 19 00
Pause 500
Command ID: CARRIER_READY
Send command: 84 A9 61 00 02 00 19 {READY_VAR}
Receive Data: 84 A9 61 00 02 00 19 00


Command ID:	CALL_START
Send	Command: 84 A9 61 00 02 00 20 02
Receive	Command:84 A9 61 00 02 00 20 00
PAUSE 50
Receive	Data:84 A9 61 00 03 30 57 00 00
Receive	Data:84 A9 61 00 02 30 54 02
Receive	Data:84 A9 61 00 04 30 50 FF FD FC
Receive	Data:84 A9 61 00 04 30 51 B7 E9 0E
Receive	Data:84 A9 61 00 05 30 52 8A AA AA A0
Receive	Data:84 A9 61 00 05 30 53 82 32 45 60
Receive	Data:84 A9 61 00 04 30 5C 77 F5 D5
Receive	Data:84 A9 61 00 02 30 27 02

Command ID:	CALL_END
Send	Command: 84 A9 61 00 01 00 21 00
Receive	Data:84 A9 61 00 02 00 21 00
Receive	Data:84 A9 61 00 02 20 17 0A
Receive	Data:84 A9 61 00 04 30 4B 00 00 00
Pause 500

Command ID: DPMR_CALLED_ID
Send command: 84 A9 61 00 05 03 52 7A AA AA A0
Receive Data: 84 A9 61 00 02 03 52 00

Command ID: DPMR_OWN_ID
Send command: 84 A9 61 00 05 03 53 72 32 45 60
Receive Data: 84 A9 61 00 02 03 53 00

Command ID: CARRIER_LOST
Send command: 84 A9 61 00 02 00 19 00
Receive Data: 84 A9 61 00 02 00 19 00
Pause 500
Command ID: CARRIER_READY
Send command: 84 A9 61 00 02 00 19 {READY_VAR}
Receive Data: 84 A9 61 00 02 00 19 00


Command ID:	CALL_START
Send	Command: 84 A9 61 00 02 00 20 02
Receive	Command:84 A9 61 00 02 00 20 00
PAUSE 50
Receive	Data:84 A9 61 00 03 30 57 00 00
Receive	Data:84 A9 61 00 02 30 54 02
Receive	Data:84 A9 61 00 04 30 50 FF FD FB
Receive	Data:84 A9 61 00 04 30 51 A1 91 EA
Receive	Data:84 A9 61 00 05 30 52 7A AA AA A0
Receive	Data:84 A9 61 00 05 30 53 72 32 45 60
Receive	Data:84 A9 61 00 04 30 5C 77 F5 D5
Receive	Data:84 A9 61 00 02 30 27 02

Command ID:	CALL_END
Send	Command: 84 A9 61 00 01 00 21 00
Receive	Data:84 A9 61 00 02 00 21 00
Receive	Data:84 A9 61 00 02 20 17 0A
Receive	Data:84 A9 61 00 04 30 4B 00 00 00
Pause 500

Command ID: DPMR_CALLED_ID
Send command: 84 A9 61 00 05 03 52 6A AA AA A0
Receive Data: 84 A9 61 00 02 03 52 00

Command ID: DPMR_OWN_ID
Send command: 84 A9 61 00 05 03 53 66 32 45 60
Receive Data: 84 A9 61 00 02 03 53 00

Command ID: CARRIER_LOST
Send command: 84 A9 61 00 02 00 19 00
Receive Data: 84 A9 61 00 02 00 19 00
Pause 500
Command ID: CARRIER_READY
Send command: 84 A9 61 00 02 00 19 {READY_VAR}
Receive Data: 84 A9 61 00 02 00 19 00


Command ID:	CALL_START
Send	Command: 84 A9 61 00 02 00 20 02
Receive	Command:84 A9 61 00 02 00 20 00
PAUSE 50
Receive	Data:84 A9 61 00 03 30 57 00 00
Receive	Data:84 A9 61 00 02 30 54 02
Receive	Data:84 A9 61 00 04 30 50 FF FD FA
Receive	Data:84 A9 61 00 04 30 51 94 2A 6E
Receive	Data:84 A9 61 00 05 30 52 6A AA AA A0
Receive	Data:84 A9 61 00 05 30 53 66 32 45 60
Receive	Data:84 A9 61 00 04 30 5C 77 F5 D5
Receive	Data:84 A9 61 00 02 30 27 02

Command ID:	CALL_END
Send	Command: 84 A9 61 00 01 00 21 00
Receive	Data:84 A9 61 00 02 00 21 00
Receive	Data:84 A9 61 00 02 20 17 0A
Receive	Data:84 A9 61 00 04 30 4B 00 00 00
Pause 500

Command ID: DPMR_CALLED_ID
Send command: 84 A9 61 00 04 03 50 FF FD F9     //BCD:5A AA AA A0
Receive Data: 84 A9 61 00 02 03 50 00

Command ID: DPMR_OWN_ID
Send command: 84 A9 61 00 05 03 53 66 32 45 60
Receive Data: 84 A9 61 00 02 03 53 00

Command ID: CARRIER_LOST
Send command: 84 A9 61 00 02 00 19 00
Receive Data: 84 A9 61 00 02 00 19 00
Pause 500
Command ID: CARRIER_READY
Send command: 84 A9 61 00 02 00 19 {READY_VAR}
Receive Data: 84 A9 61 00 02 00 19 00


Command ID:	CALL_START
Send	Command: 84 A9 61 00 02 00 20 02
Receive	Command:84 A9 61 00 02 00 20 00
PAUSE 50
Receive	Data:84 A9 61 00 03 30 57 00 00
Receive	Data:84 A9 61 00 02 30 54 02
Receive	Data:84 A9 61 00 04 30 50 FF FD F9
Receive	Data:84 A9 61 00 04 30 51 94 2A 6E
Receive	Data:84 A9 61 00 05 30 52 5A AA AA A0
Receive	Data:84 A9 61 00 05 30 53 66 32 45 60
Receive	Data:84 A9 61 00 04 30 5C 77 F5 D5
Receive	Data:84 A9 61 00 02 30 27 05

Command ID:	CALL_END
Send	Command: 84 A9 61 00 01 00 21 00
Receive	Data:84 A9 61 00 02 00 21 00
Receive	Data:84 A9 61 00 02 20 17 0A
Receive	Data:84 A9 61 00 04 30 4B 00 00 00
Pause 1000

Command ID: DPMR_CALLED_ID
Send command: 84 A9 61 00 04 03 50 FF FD F4     //BCD:0A AA AA A0
Receive Data: 84 A9 61 00 02 03 50 00

Command ID: DPMR_OWN_ID
Send command: 84 A9 61 00 05 03 53 06 32 45 60
Receive Data: 84 A9 61 00 02 03 53 00

Command ID: CARRIER_LOST
Send command: 84 A9 61 00 02 00 19 00
Receive Data: 84 A9 61 00 02 00 19 00
Pause 500
Command ID: CARRIER_READY
Send command: 84 A9 61 00 02 00 19 {READY_VAR}
Receive Data: 84 A9 61 00 02 00 19 00


Command ID:	CALL_START
Send	Command: 84 A9 61 00 02 00 20 02
Receive	Command:84 A9 61 00 02 00 20 00
PAUSE 50
Receive	Data:84 A9 61 00 03 30 57 00 00
Receive	Data:84 A9 61 00 02 30 54 02
Receive	Data:84 A9 61 00 04 30 50 FF FD F4
Receive	Data:84 A9 61 00 04 30 51 0E 1F 96
Receive	Data:84 A9 61 00 05 30 52 0A AA AA A0
Receive	Data:84 A9 61 00 05 30 53 06 32 45 60
Receive	Data:84 A9 61 00 04 30 5C 77 F5 D5
Receive	Data:84 A9 61 00 02 30 27 02

Command ID:	CALL_END
Send	Command: 84 A9 61 00 01 00 21 00
Receive	Data:84 A9 61 00 02 00 21 00
Receive	Data:84 A9 61 00 02 20 17 0A
Receive	Data:84 A9 61 00 04 30 4B 00 00 00
Pause 1000

Command ID: DPMR_CALLED_ID
Send command: 84 A9 61 00 04 03 50 FF FD F5     //BCD:1A AA AA A0
Receive Data: 84 A9 61 00 02 03 50 00

Command ID: DPMR_OWN_ID
Send command: 84 A9 61 00 05 03 53 16 32 45 60
Receive Data: 84 A9 61 00 02 03 53 00

Command ID: CARRIER_LOST
Send command: 84 A9 61 00 02 00 19 00
Receive Data: 84 A9 61 00 02 00 19 00
Pause 500
Command ID: CARRIER_READY
Send command: 84 A9 61 00 02 00 19 {READY_VAR}
Receive Data: 84 A9 61 00 02 00 19 00


Command ID:	CALL_START
Send	Command: 84 A9 61 00 02 00 20 02
Receive	Command:84 A9 61 00 02 00 20 00
PAUSE 50
Receive	Data:84 A9 61 00 03 30 57 00 00
Receive	Data:84 A9 61 00 02 30 54 02
Receive	Data:84 A9 61 00 04 30 50 FF FD F5
Receive	Data:84 A9 61 00 04 30 51 24 76 BA
Receive	Data:84 A9 61 00 05 30 52 1A AA AA A0
Receive	Data:84 A9 61 00 05 30 53 16 32 45 60
Receive	Data:84 A9 61 00 04 30 5C 77 F5 D5
Receive	Data:84 A9 61 00 02 30 27 02

Command ID:	CALL_END
Send	Command: 84 A9 61 00 01 00 21 00
Receive	Data:84 A9 61 00 02 00 21 00
Receive	Data:84 A9 61 00 02 20 17 0A
Receive	Data:84 A9 61 00 04 30 4B 00 00 00
Pause 1000

Command ID: DPMR_CALLED_ID
Send command: 84 A9 61 00 04 03 50 FF FD F6     //BCD:2A AA AA A0
Receive Data: 84 A9 61 00 02 03 50 00

Command ID: DPMR_OWN_ID
Send command: 84 A9 61 00 05 03 53 26 32 45 60
Receive Data: 84 A9 61 00 02 03 53 00

Command ID: CARRIER_LOST
Send command: 84 A9 61 00 02 00 19 00
Receive Data: 84 A9 61 00 02 00 19 00
Pause 500
Command ID: CARRIER_READY
Send command: 84 A9 61 00 02 00 19 {READY_VAR}
Receive Data: 84 A9 61 00 02 00 19 00


Command ID:	CALL_START
Send	Command: 84 A9 61 00 02 00 20 02
Receive	Command:84 A9 61 00 02 00 20 00
PAUSE 50
Receive	Data:84 A9 61 00 03 30 57 00 00
Receive	Data:84 A9 61 00 02 30 54 02
Receive	Data:84 A9 61 00 04 30 50 FF FD F6
Receive	Data:84 A9 61 00 04 30 51 3A CD DE
Receive	Data:84 A9 61 00 05 30 52 2A AA AA A0
Receive	Data:84 A9 61 00 05 30 53 26 32 45 60
Receive	Data:84 A9 61 00 04 30 5C 77 F5 D5
Receive	Data:84 A9 61 00 02 30 27 02

Command ID:	CALL_END
Send	Command: 84 A9 61 00 01 00 21 00
Receive	Data:84 A9 61 00 02 00 21 00
Receive	Data:84 A9 61 00 02 20 17 0A
Receive	Data:84 A9 61 00 04 30 4B 00 00 00
Pause 1000

Command ID: DPMR_CALLED_ID
Send command: 84 A9 61 00 04 03 50 FF FD F7     //BCD:3A AA AA A0
Receive Data: 84 A9 61 00 02 03 50 00

Command ID: DPMR_OWN_ID
Send command: 84 A9 61 00 05 03 53 36 32 45 60
Receive Data: 84 A9 61 00 02 03 53 00

Command ID: CARRIER_LOST
Send command: 84 A9 61 00 02 00 19 00
Receive Data: 84 A9 61 00 02 00 19 00
Pause 500
Command ID: CARRIER_READY
Send command: 84 A9 61 00 02 00 19 {READY_VAR}
Receive Data: 84 A9 61 00 02 00 19 00


Command ID:	CALL_START
Send	Command: 84 A9 61 00 02 00 20 02
Receive	Command:84 A9 61 00 02 00 20 00
PAUSE 50
Receive	Data:84 A9 61 00 03 30 57 00 00
Receive	Data:84 A9 61 00 02 30 54 02
Receive	Data:84 A9 61 00 04 30 50 FF FD F7
Receive	Data:84 A9 61 00 04 30 51 51 25 02
Receive	Data:84 A9 61 00 05 30 52 3A AA AA A0
Receive	Data:84 A9 61 00 05 30 53 36 32 45 60
Receive	Data:84 A9 61 00 04 30 5C 77 F5 D5
Receive	Data:84 A9 61 00 02 30 27 02

Command ID:	CALL_END
Send	Command: 84 A9 61 00 01 00 21 00
Receive	Data:84 A9 61 00 02 00 21 00
Receive	Data:84 A9 61 00 02 20 17 0A
Receive	Data:84 A9 61 00 04 30 4B 00 00 00
Pause 1000

Command ID: DPMR_CALLED_ID
Send command: 84 A9 61 00 04 03 50 FF FD F8     //BCD:4A AA AA A0
Receive Data: 84 A9 61 00 02 03 50 00

Command ID: DPMR_OWN_ID
Send command: 84 A9 61 00 05 03 53 46 32 45 60
Receive Data: 84 A9 61 00 02 03 53 00

Command ID: CARRIER_LOST
Send command: 84 A9 61 00 02 00 19 00
Receive Data: 84 A9 61 00 02 00 19 00
Pause 500
Command ID: CARRIER_READY
Send command: 84 A9 61 00 02 00 19 {READY_VAR}
Receive Data: 84 A9 61 00 02 00 19 00


Command ID:	CALL_START
Send	Command: 84 A9 61 00 02 00 20 02
Receive	Command:84 A9 61 00 02 00 20 00
PAUSE 50
Receive	Data:84 A9 61 00 03 30 57 00 00
Receive	Data:84 A9 61 00 02 30 54 02
Receive	Data:84 A9 61 00 04 30 50 FF FD F8
Receive	Data:84 A9 61 00 04 30 51 67 7C 26
Receive	Data:84 A9 61 00 05 30 52 4A AA AA A0
Receive	Data:84 A9 61 00 05 30 53 46 32 45 60
Receive	Data:84 A9 61 00 04 30 5C 77 F5 D5
Receive	Data:84 A9 61 00 02 30 27 02

Command ID:	CALL_END
Send	Command: 84 A9 61 00 01 00 21 00
Receive	Data:84 A9 61 00 02 00 21 00
Receive	Data:84 A9 61 00 02 20 17 0A
Receive	Data:84 A9 61 00 04 30 4B 00 00 00
Pause 1000

Command ID: DPMR_CALLED_ID
Send command: 84 A9 61 00 04 03 50 FF FD FE     //BCD:AA AA AA A0
Receive Data: 84 A9 61 00 02 03 50 00

Command ID: DPMR_OWN_ID
Send command: 84 A9 61 00 05 03 53 06 33 88 90
Receive Data: 84 A9 61 00 02 03 53 00

Command ID: CARRIER_LOST
Send command: 84 A9 61 00 02 00 19 00
Receive Data: 84 A9 61 00 02 00 19 00
Pause 500
Command ID: CARRIER_READY
Send command: 84 A9 61 00 02 00 19 {READY_VAR}
Receive Data: 84 A9 61 00 02 00 19 00


Command ID:	CALL_START
Send	Command: 84 A9 61 00 02 00 20 02
Receive	Command:84 A9 61 00 02 00 20 00
PAUSE 50
Receive	Data:84 A9 61 00 03 30 57 00 00
Receive	Data:84 A9 61 00 02 30 54 02
Receive	Data:84 A9 61 00 04 30 50 FF FD FE
Receive	Data:84 A9 61 00 04 30 51 0E 26 D1
Receive	Data:84 A9 61 00 05 30 52 AA AA AA A0
Receive	Data:84 A9 61 00 05 30 53 06 33 88 90
Receive	Data:84 A9 61 00 04 30 5C 77 F5 D5
Receive	Data:84 A9 61 00 02 30 27 02

Command ID:	CALL_END
Send	Command: 84 A9 61 00 01 00 21 00
Receive	Data:84 A9 61 00 02 00 21 00
Receive	Data:84 A9 61 00 02 20 17 0A
Receive	Data:84 A9 61 00 04 30 4B 00 00 00
Pause 1000

//////////////////////////////

Command ID: PROTOCOL_OPTION  
Send command: 84 A9 61 00 02 00 55 8a  //NEW all call**************************************************************
Receive Data: 84 A9 61 00 02 00 55 00


Command ID: DPMR_CALLED_ID
Send command: 84 A9 61 00 04 03 50 F8 33 A5 //bcd:9A AA AA A0
Receive Data: 84 A9 61 00 02 03 50 00

Command ID: DPMR_OWN_ID
Send command: 84 A9 61 00 05 03 53 92 34 56 70
Receive Data: 84 A9 61 00 02 03 53 00

Command ID: CARRIER_LOST
Send command: 84 A9 61 00 02 00 19 00
Receive Data: 84 A9 61 00 02 00 19 00
Pause 500
Command ID: CARRIER_READY
Send command: 84 A9 61 00 02 00 19 {READY_VAR}
Receive Data: 84 A9 61 00 02 00 19 00


Command ID:	CALL_START
Send	Command: 84 A9 61 00 02 00 20 02
Receive	Command:84 A9 61 00 02 00 20 00
PAUSE 50
Receive	Data:84 A9 61 00 03 30 57 00 00
Receive	Data:84 A9 61 00 02 30 54 02
Receive	Data:84 A9 61 00 04 30 50 F8 33 A5
Receive	Data:84 A9 61 00 04 30 51 CE 4B 1D
Receive	Data:84 A9 61 00 05 30 52 9A AA AA A0
Receive	Data:84 A9 61 00 05 30 53 92 34 56 70
Receive	Data:84 A9 61 00 04 30 5C 77 F5 D5
Receive	Data:84 A9 61 00 02 30 27 02

Command ID:	CALL_END
Send	Command: 84 A9 61 00 01 00 21 00
Receive	Data:84 A9 61 00 02 00 21 00
Receive	Data:84 A9 61 00 02 20 17 0A
Receive	Data:84 A9 61 00 04 30 4B 00 00 00
Pause 500

Command ID: DPMR_CALLED_ID
Send command: 84 A9 61 00 04 03 50 F8 33 A4 //bcd:8A AA AA A0
Receive Data: 84 A9 61 00 02 03 50 00

Command ID: DPMR_OWN_ID
Send command: 84 A9 61 00 05 03 53 82 32 45 60
Receive Data: 84 A9 61 00 02 03 53 00

Command ID: CARRIER_LOST
Send command: 84 A9 61 00 02 00 19 00
Receive Data: 84 A9 61 00 02 00 19 00
Pause 500
Command ID: CARRIER_READY
Send command: 84 A9 61 00 02 00 19 {READY_VAR}
Receive Data: 84 A9 61 00 02 00 19 00


Command ID:	CALL_START
Send	Command: 84 A9 61 00 02 00 20 02
Receive	Command:84 A9 61 00 02 00 20 00
PAUSE 50
Receive	Data:84 A9 61 00 03 30 57 00 00
Receive	Data:84 A9 61 00 02 30 54 02
Receive	Data:84 A9 61 00 04 30 50 F8 33 A4
Receive	Data:84 A9 61 00 04 30 51 B7 E9 0E
Receive	Data:84 A9 61 00 05 30 52 8A AA AA A0
Receive	Data:84 A9 61 00 05 30 53 82 32 45 60
Receive	Data:84 A9 61 00 04 30 5C 77 F5 D5
Receive	Data:84 A9 61 00 02 30 27 02

Command ID:	CALL_END
Send	Command: 84 A9 61 00 01 00 21 00
Receive	Data:84 A9 61 00 02 00 21 00
Receive	Data:84 A9 61 00 02 20 17 0A
Receive	Data:84 A9 61 00 04 30 4B 00 00 00
Pause 500

Command ID: DPMR_CALLED_ID
Send command: 84 A9 61 00 05 03 52 7A AA AA A0
Receive Data: 84 A9 61 00 02 03 52 00

Command ID: DPMR_OWN_ID
Send command: 84 A9 61 00 05 03 53 72 32 45 60
Receive Data: 84 A9 61 00 02 03 53 00

Command ID: CARRIER_LOST
Send command: 84 A9 61 00 02 00 19 00
Receive Data: 84 A9 61 00 02 00 19 00
Pause 500
Command ID: CARRIER_READY
Send command: 84 A9 61 00 02 00 19 {READY_VAR}
Receive Data: 84 A9 61 00 02 00 19 00


Command ID:	CALL_START
Send	Command: 84 A9 61 00 02 00 20 02
Receive	Command:84 A9 61 00 02 00 20 00
PAUSE 50
Receive	Data:84 A9 61 00 03 30 57 00 00
Receive	Data:84 A9 61 00 02 30 54 02
Receive	Data:84 A9 61 00 04 30 50 F8 33 A3
Receive	Data:84 A9 61 00 04 30 51 A1 91 EA
Receive	Data:84 A9 61 00 05 30 52 7A AA AA A0
Receive	Data:84 A9 61 00 05 30 53 72 32 45 60
Receive	Data:84 A9 61 00 04 30 5C 77 F5 D5
Receive	Data:84 A9 61 00 02 30 27 02

Command ID:	CALL_END
Send	Command: 84 A9 61 00 01 00 21 00
Receive	Data:84 A9 61 00 02 00 21 00
Receive	Data:84 A9 61 00 02 20 17 0A
Receive	Data:84 A9 61 00 04 30 4B 00 00 00
Pause 500

Command ID: DPMR_CALLED_ID
Send command: 84 A9 61 00 05 03 52 6A AA AA A0
Receive Data: 84 A9 61 00 02 03 52 00

Command ID: DPMR_OWN_ID
Send command: 84 A9 61 00 05 03 53 66 32 45 60
Receive Data: 84 A9 61 00 02 03 53 00

Command ID: CARRIER_LOST
Send command: 84 A9 61 00 02 00 19 00
Receive Data: 84 A9 61 00 02 00 19 00
Pause 500
Command ID: CARRIER_READY
Send command: 84 A9 61 00 02 00 19 {READY_VAR}
Receive Data: 84 A9 61 00 02 00 19 00


Command ID:	CALL_START
Send	Command: 84 A9 61 00 02 00 20 02
Receive	Command:84 A9 61 00 02 00 20 00
PAUSE 50
Receive	Data:84 A9 61 00 03 30 57 00 00
Receive	Data:84 A9 61 00 02 30 54 02
Receive	Data:84 A9 61 00 04 30 50 F8 33 A2
Receive	Data:84 A9 61 00 04 30 51 94 2A 6E
Receive	Data:84 A9 61 00 05 30 52 6A AA AA A0
Receive	Data:84 A9 61 00 05 30 53 66 32 45 60
Receive	Data:84 A9 61 00 04 30 5C 77 F5 D5
Receive	Data:84 A9 61 00 02 30 27 02

Command ID:	CALL_END
Send	Command: 84 A9 61 00 01 00 21 00
Receive	Data:84 A9 61 00 02 00 21 00
Receive	Data:84 A9 61 00 02 20 17 0A
Receive	Data:84 A9 61 00 04 30 4B 00 00 00
Pause 500

Command ID: DPMR_CALLED_ID
Send command: 84 A9 61 00 04 03 50 F8 33 A1     //BCD:5A AA AA A0
Receive Data: 84 A9 61 00 02 03 50 00

Command ID: DPMR_OWN_ID
Send command: 84 A9 61 00 05 03 53 66 32 45 60
Receive Data: 84 A9 61 00 02 03 53 00

Command ID: CARRIER_LOST
Send command: 84 A9 61 00 02 00 19 00
Receive Data: 84 A9 61 00 02 00 19 00
Pause 500
Command ID: CARRIER_READY
Send command: 84 A9 61 00 02 00 19 {READY_VAR}
Receive Data: 84 A9 61 00 02 00 19 00


Command ID:	CALL_START
Send	Command: 84 A9 61 00 02 00 20 02
Receive	Command:84 A9 61 00 02 00 20 00
PAUSE 50
Receive	Data:84 A9 61 00 03 30 57 00 00
Receive	Data:84 A9 61 00 02 30 54 02
Receive	Data:84 A9 61 00 04 30 50 F8 33 A1
Receive	Data:84 A9 61 00 04 30 51 94 2A 6E
Receive	Data:84 A9 61 00 05 30 52 5A AA AA A0
Receive	Data:84 A9 61 00 05 30 53 66 32 45 60
Receive	Data:84 A9 61 00 04 30 5C 77 F5 D5
Receive	Data:84 A9 61 00 02 30 27 05

Command ID:	CALL_END
Send	Command: 84 A9 61 00 01 00 21 00
Receive	Data:84 A9 61 00 02 00 21 00
Receive	Data:84 A9 61 00 02 20 17 0A
Receive	Data:84 A9 61 00 04 30 4B 00 00 00
Pause 1000

Command ID: DPMR_CALLED_ID
Send command: 84 A9 61 00 04 03 50 F8 33 9C     //BCD:0A AA AA A0
Receive Data: 84 A9 61 00 02 03 50 00

Command ID: DPMR_OWN_ID
Send command: 84 A9 61 00 05 03 53 06 32 45 60
Receive Data: 84 A9 61 00 02 03 53 00

Command ID: CARRIER_LOST
Send command: 84 A9 61 00 02 00 19 00
Receive Data: 84 A9 61 00 02 00 19 00
Pause 500
Command ID: CARRIER_READY
Send command: 84 A9 61 00 02 00 19 {READY_VAR}
Receive Data: 84 A9 61 00 02 00 19 00


Command ID:	CALL_START
Send	Command: 84 A9 61 00 02 00 20 02
Receive	Command:84 A9 61 00 02 00 20 00
PAUSE 50
Receive	Data:84 A9 61 00 03 30 57 00 00
Receive	Data:84 A9 61 00 02 30 54 02
Receive	Data:84 A9 61 00 04 30 50 F8 33 9C
Receive	Data:84 A9 61 00 04 30 51 0E 1F 96
Receive	Data:84 A9 61 00 05 30 52 0A AA AA A0
Receive	Data:84 A9 61 00 05 30 53 06 32 45 60
Receive	Data:84 A9 61 00 04 30 5C 77 F5 D5
Receive	Data:84 A9 61 00 02 30 27 02

Command ID:	CALL_END
Send	Command: 84 A9 61 00 01 00 21 00
Receive	Data:84 A9 61 00 02 00 21 00
Receive	Data:84 A9 61 00 02 20 17 0A
Receive	Data:84 A9 61 00 04 30 4B 00 00 00
Pause 1000

Command ID: DPMR_CALLED_ID
Send command: 84 A9 61 00 04 03 50 F8 33 9D     //BCD:1A AA AA A0
Receive Data: 84 A9 61 00 02 03 50 00

Command ID: DPMR_OWN_ID
Send command: 84 A9 61 00 05 03 53 16 32 45 60
Receive Data: 84 A9 61 00 02 03 53 00

Command ID: CARRIER_LOST
Send command: 84 A9 61 00 02 00 19 00
Receive Data: 84 A9 61 00 02 00 19 00
Pause 500
Command ID: CARRIER_READY
Send command: 84 A9 61 00 02 00 19 {READY_VAR}
Receive Data: 84 A9 61 00 02 00 19 00


Command ID:	CALL_START
Send	Command: 84 A9 61 00 02 00 20 02
Receive	Command:84 A9 61 00 02 00 20 00
PAUSE 50
Receive	Data:84 A9 61 00 03 30 57 00 00
Receive	Data:84 A9 61 00 02 30 54 02
Receive	Data:84 A9 61 00 04 30 50 F8 33 9D
Receive	Data:84 A9 61 00 04 30 51 24 76 BA
Receive	Data:84 A9 61 00 05 30 52 1A AA AA A0
Receive	Data:84 A9 61 00 05 30 53 16 32 45 60
Receive	Data:84 A9 61 00 04 30 5C 77 F5 D5
Receive	Data:84 A9 61 00 02 30 27 02

Command ID:	CALL_END
Send	Command: 84 A9 61 00 01 00 21 00
Receive	Data:84 A9 61 00 02 00 21 00
Receive	Data:84 A9 61 00 02 20 17 0A
Receive	Data:84 A9 61 00 04 30 4B 00 00 00
Pause 1000

Command ID: DPMR_CALLED_ID
Send command: 84 A9 61 00 04 03 50 F8 33 9E     //BCD:2A AA AA A0
Receive Data: 84 A9 61 00 02 03 50 00

Command ID: DPMR_OWN_ID
Send command: 84 A9 61 00 05 03 53 26 32 45 60
Receive Data: 84 A9 61 00 02 03 53 00

Command ID: CARRIER_LOST
Send command: 84 A9 61 00 02 00 19 00
Receive Data: 84 A9 61 00 02 00 19 00
Pause 500
Command ID: CARRIER_READY
Send command: 84 A9 61 00 02 00 19 {READY_VAR}
Receive Data: 84 A9 61 00 02 00 19 00


Command ID:	CALL_START
Send	Command: 84 A9 61 00 02 00 20 02
Receive	Command:84 A9 61 00 02 00 20 00
PAUSE 50
Receive	Data:84 A9 61 00 03 30 57 00 00
Receive	Data:84 A9 61 00 02 30 54 02
Receive	Data:84 A9 61 00 04 30 50 F8 33 9E
Receive	Data:84 A9 61 00 04 30 51 3A CD DE
Receive	Data:84 A9 61 00 05 30 52 2A AA AA A0
Receive	Data:84 A9 61 00 05 30 53 26 32 45 60
Receive	Data:84 A9 61 00 04 30 5C 77 F5 D5
Receive	Data:84 A9 61 00 02 30 27 02

Command ID:	CALL_END
Send	Command: 84 A9 61 00 01 00 21 00
Receive	Data:84 A9 61 00 02 00 21 00
Receive	Data:84 A9 61 00 02 20 17 0A
Receive	Data:84 A9 61 00 04 30 4B 00 00 00
Pause 1000

Command ID: DPMR_CALLED_ID
Send command: 84 A9 61 00 04 03 50 F8 33 9F     //BCD:3A AA AA A0
Receive Data: 84 A9 61 00 02 03 50 00

Command ID: DPMR_OWN_ID
Send command: 84 A9 61 00 05 03 53 36 32 45 60
Receive Data: 84 A9 61 00 02 03 53 00

Command ID: CARRIER_LOST
Send command: 84 A9 61 00 02 00 19 00
Receive Data: 84 A9 61 00 02 00 19 00
Pause 500
Command ID: CARRIER_READY
Send command: 84 A9 61 00 02 00 19 {READY_VAR}
Receive Data: 84 A9 61 00 02 00 19 00


Command ID:	CALL_START
Send	Command: 84 A9 61 00 02 00 20 02
Receive	Command:84 A9 61 00 02 00 20 00
PAUSE 50
Receive	Data:84 A9 61 00 03 30 57 00 00
Receive	Data:84 A9 61 00 02 30 54 02
Receive	Data:84 A9 61 00 04 30 50 F8 33 9F
Receive	Data:84 A9 61 00 04 30 51 51 25 02
Receive	Data:84 A9 61 00 05 30 52 3A AA AA A0
Receive	Data:84 A9 61 00 05 30 53 36 32 45 60
Receive	Data:84 A9 61 00 04 30 5C 77 F5 D5
Receive	Data:84 A9 61 00 02 30 27 02

Command ID:	CALL_END
Send	Command: 84 A9 61 00 01 00 21 00
Receive	Data:84 A9 61 00 02 00 21 00
Receive	Data:84 A9 61 00 02 20 17 0A
Receive	Data:84 A9 61 00 04 30 4B 00 00 00
Pause 1000

Command ID: DPMR_CALLED_ID
Send command: 84 A9 61 00 04 03 50 F8 33 A0     //BCD:4A AA AA A0
Receive Data: 84 A9 61 00 02 03 50 00

Command ID: DPMR_OWN_ID
Send command: 84 A9 61 00 05 03 53 46 32 45 60
Receive Data: 84 A9 61 00 02 03 53 00

Command ID: CARRIER_LOST
Send command: 84 A9 61 00 02 00 19 00
Receive Data: 84 A9 61 00 02 00 19 00
Pause 500
Command ID: CARRIER_READY
Send command: 84 A9 61 00 02 00 19 {READY_VAR}
Receive Data: 84 A9 61 00 02 00 19 00


Command ID:	CALL_START
Send	Command: 84 A9 61 00 02 00 20 02
Receive	Command:84 A9 61 00 02 00 20 00
PAUSE 50
Receive	Data:84 A9 61 00 03 30 57 00 00
Receive	Data:84 A9 61 00 02 30 54 02
Receive	Data:84 A9 61 00 04 30 50 F8 33 A0
Receive	Data:84 A9 61 00 04 30 51 67 7C 26
Receive	Data:84 A9 61 00 05 30 52 4A AA AA A0
Receive	Data:84 A9 61 00 05 30 53 46 32 45 60
Receive	Data:84 A9 61 00 04 30 5C 77 F5 D5
Receive	Data:84 A9 61 00 02 30 27 02

Command ID:	CALL_END
Send	Command: 84 A9 61 00 01 00 21 00
Receive	Data:84 A9 61 00 02 00 21 00
Receive	Data:84 A9 61 00 02 20 17 0A
Receive	Data:84 A9 61 00 04 30 4B 00 00 00
Pause 1000

Command ID: DPMR_CALLED_ID
Send command: 84 A9 61 00 04 03 50 F8 33 A6     //BCD:AA AA AA A0
Receive Data: 84 A9 61 00 02 03 50 00

Command ID: DPMR_OWN_ID
Send command: 84 A9 61 00 05 03 53 06 33 88 90
Receive Data: 84 A9 61 00 02 03 53 00

Command ID: CARRIER_LOST
Send command: 84 A9 61 00 02 00 19 00
Receive Data: 84 A9 61 00 02 00 19 00
Pause 500
Command ID: CARRIER_READY
Send command: 84 A9 61 00 02 00 19 {READY_VAR}
Receive Data: 84 A9 61 00 02 00 19 00


Command ID:	CALL_START
Send	Command: 84 A9 61 00 02 00 20 02
Receive	Command:84 A9 61 00 02 00 20 00
PAUSE 50
Receive	Data:84 A9 61 00 03 30 57 00 00
Receive	Data:84 A9 61 00 02 30 54 02
Receive	Data:84 A9 61 00 04 30 50 F8 33 A6
Receive	Data:84 A9 61 00 04 30 51 0E 26 D1
Receive	Data:84 A9 61 00 05 30 52 AA AA AA A0
Receive	Data:84 A9 61 00 05 30 53 06 33 88 90
Receive	Data:84 A9 61 00 04 30 5C 77 F5 D5
Receive	Data:84 A9 61 00 02 30 27 02

Command ID:	CALL_END
Send	Command: 84 A9 61 00 01 00 21 00
Receive	Data:84 A9 61 00 02 00 21 00
Receive	Data:84 A9 61 00 02 20 17 0A
Receive	Data:84 A9 61 00 04 30 4B 00 00 00
Pause 1000

