//Verison=2.2
//Example,Don't Delete flowing text!
//Button NIMI // Generator NIMI 
//Button NIMI 100 // Generator NIMI and Delay 100ms, 100 not is nessary
//Button INT0 // Generator INT0 and Delay 200ms
//Button RESETAMBE3000
//Button RESET3252
//Send 1 command, Receive 2 response with one is not verify.
//Command ID: CARRIER_LOST // necessary!
//Summary  // not essential, 
//Send command: 61 00 02 00 19 00 // necessary!
//Pause=300 // not essential, unit: ms; Pause 300ms after Send command
//Timeout=100 // not essential, unit: ms; if not receive '84 A9 61 ...' in 100ms after send command, Timeout error will happen!
//*Receive Data: 61 00 02 51 19 00 // not essential, receive but not verify
//Receive Data: 61 00 02 51 19 20 // not essential, receive and verify 
//.Set x = AA B0  -- Define var x ; Added in ver2.2
// ... 61 00 02 00 19 {x}   --- use the defined var, The {x} will be replaced with AA B0 
//
.Set READY_VAR = 01
Command ID:	VOCODER_SEL
Send	Command: 84 A9 61 00 02 00 10 01
Receive	Command:84 A9 61 00 02 00 10 00
PAUSE 4000
Command ID:	DPMR_CC
Send	Command: 84 A9 61 00 04 03 5C 77 F5 D5
Receive	Command:84 A9 61 00 02 03 5C 00
Command ID: WORK_MODE_DUPLEX
Send command: 84 A9 61 00 04 00 18 03 00 00
Receive Data: 84 A9 61 00 02 00 18 00
Command ID: PROCESS_MODE
Send command: 84 A9 61 00 02 00 1A 03
Receive Data: 84 A9 61 00 02 00 1A 00
Command ID:	ADDRESSING_MODE
Send	Command: 84 A9 61 00 02 03 28 01
Receive	Command:84 A9 61 00 02 03 28 00
Command ID: DPMR_CALLED_ID
Send command: 84 A9 61 00 05 03 52 12 34 56 70
Receive Data: 84 A9 61 00 02 03 52 00
Command ID: DPMR_OWN_ID
Send command: 84 A9 61 00 05 03 53 12 34 56 70
Receive Data: 84 A9 61 00 02 03 53 00
Command ID:	REPORT_FIELD
Send	Command: 84 A9 61 00 02 00 1D 7f
Receive	Command:84 A9 61 00 02 00 1D 00
Command ID: DPMR_HT_CI
Send command: 84 A9 61 00 03 03 57 00 00
Receive Data: 84 A9 61 00 02 03 57 00
Command ID: CARRIER_LOST
Send command: 84 A9 61 00 02 00 19 00
Receive Data: 84 A9 61 00 02 00 19 00
Pause 500
Command ID: CARRIER_READY
Send command: 84 A9 61 00 02 00 19 {READY_VAR}
Receive Data: 84 A9 61 00 02 00 19 00

//FOR DPMR VOICE CALL
Command ID:	CALL_START
Send	Command: 84 A9 61 00 02 00 20 02
Receive	Command:84 A9 61 00 02 00 20 00


Receive	Data:84 A9 61 00 03 30 57 00 00
Receive	Data:84 A9 61 00 02 30 54 02
Receive	Data:84 A9 61 00 04 30 50 1B 91 FD
Receive	Data:84 A9 61 00 04 30 51 1B 91 FD
Receive	Data:84 A9 61 00 05 30 52 12 34 56 70
Receive	Data:84 A9 61 00 05 30 53 12 34 56 70
Receive	Data:84 A9 61 00 04 30 5C 77 F5 D5
Receive	Data:84 A9 61 00 02 30 27 00

Pause 3000
Command ID:	CALL_END
Send	Command: 84 A9 61 00 01 00 21 
Receive	Command:84 A9 61 00 02 00 21 00
Receive	Command:84 A9 61 00 02 20 17 0A
Receive	 Data:84 A9 61 00 04 30 4B 00 00 00
Pause 2000

Command ID: CARRIER_LOST
Send command: 84 A9 61 00 02 00 19 00
Receive Data: 84 A9 61 00 02 00 19 00
Pause 500
Command ID: CARRIER_READY
Send command: 84 A9 61 00 02 00 19 {READY_VAR}
Receive Data: 84 A9 61 00 02 00 19 00

//FOR NDR VOICE CALL 
Command ID: PROTOCOL_OPTION  
Send command: 84 A9 61 00 02 00 55 40
Receive Data: 84 A9 61 00 02 00 55 00

Command ID: DPMR_HT_CI
Send command: 84 A9 61 00 03 03 57 00 00
Receive Data: 84 A9 61 00 02 03 57 00

Command ID:	CALL_START
Send	Command: 84 A9 61 00 02 00 20 02
Receive	Command:84 A9 61 00 02 00 20 00

Receive	Data:84 A9 61 00 03 30 57 00 00
Receive	Data:84 A9 61 00 02 30 54 02
Receive	Data:84 A9 61 00 04 30 50 1B 91 FD
Receive	Data:84 A9 61 00 04 30 51 1B 91 FD
Receive	Data:84 A9 61 00 05 30 52 12 34 56 70
Receive	Data:84 A9 61 00 05 30 53 12 34 56 70
Receive	Data:84 A9 61 00 04 30 5C 77 F5 D5
Receive	Data:84 A9 61 00 02 30 27 00

Pause 3000
Command ID:	CALL_END
Send	Command: 84 A9 61 00 01 00 21 
Receive	Command:84 A9 61 00 02 00 21 00
Receive	Command:84 A9 61 00 02 20 17 0A
Receive	Data:84 A9 61 00 04 30 4B 00 00 00
Pause 1000

Command ID: CARRIER_LOST
Send command: 84 A9 61 00 02 00 19 00
Receive Data: 84 A9 61 00 02 00 19 00
Pause 500
Command ID: CARRIER_READY
Send command: 84 A9 61 00 02 00 19 {READY_VAR}
Receive Data: 84 A9 61 00 02 00 19 00

Command ID:	SCRAMBLER_SEED
Send	Command: 84 A9 61 00 04 00 2A 04 C0 80
Receive	Data:84 A9 61 00 02 00 2A 00

//FOR NDR ENCRYPT VOICE CALL 
Command ID: DPMR_HT_CI
Send command: 84 A9 61 00 03 03 57 00 01
Receive Data: 84 A9 61 00 02 03 57 00



Command ID:	CALL_START
Send	Command: 84 A9 61 00 02 00 20 02
Receive	Command:84 A9 61 00 02 00 20 00

Receive	Data:84 A9 61 00 03 30 57 00 01
Receive	Data:84 A9 61 00 02 30 54 02
Receive	Data:84 A9 61 00 04 30 50 1B 91 FD
Receive	Data:84 A9 61 00 04 30 51 1B 91 FD
Receive	Data:84 A9 61 00 05 30 52 12 34 56 70
Receive	Data:84 A9 61 00 05 30 53 12 34 56 70
Receive	Data:84 A9 61 00 04 30 5C 77 F5 D5
Receive	Data:84 A9 61 00 02 30 27 00

Pause 2000
Command ID:	SCRAMBLER_SEED   //CHANGE SEED
Send	Command: 84 A9 61 00 04 00 2A 04 A0 80
Receive	Data:84 A9 61 00 02 00 2A 00
Pause 2000
Command ID:	CALL_END
Send	Command: 84 A9 61 00 01 00 21 
Receive	Command:84 A9 61 00 02 00 21 00
Receive	Command:84 A9 61 00 02 20 17 0A
Receive	Data:84 A9 61 00 04 30 4B 00 00 00
Pause 1000
Command ID: CARRIER_LOST
Send command: 84 A9 61 00 02 00 19 00
Receive Data: 84 A9 61 00 02 00 19 00
Pause 500
Command ID:	CALL_START  //FOR CCH ENCRYPT
Send	Command: 84 A9 61 00 02 00 20 02
Receive	Command:84 A9 61 00 02 00 20 00
Pause 1000
Command ID: CARRIER_READY
Send command: 84 A9 61 00 02 00 19 {READY_VAR}
Receive Data: 84 A9 61 00 02 00 19 00

Receive	Data:84 A9 61 00 02 30 54 02
Receive	Data:84 A9 61 00 04 30 50 1B 91 FD
Receive	Data:84 A9 61 00 04 30 51 1B 91 FD
Receive	Data:84 A9 61 00 05 30 52 12 34 56 70
Receive	Data:84 A9 61 00 05 30 53 12 34 56 70
Receive	Data:84 A9 61 00 04 30 5C 77 F5 D5
Receive	Data:84 A9 61 00 02 30 27 00

Pause 3000
Command ID:	CALL_END
Send	Command: 84 A9 61 00 01 00 21 
Receive	Command:84 A9 61 00 02 00 21 00
Receive	Command:84 A9 61 00 02 20 17 0A
Receive	Data:84 A9 61 00 04 30 4B 00 00 00

Pause 1000
Command ID: CARRIER_LOST
Send command: 84 A9 61 00 02 00 19 00
Receive Data: 84 A9 61 00 02 00 19 00

