//Verison=2.2
//Example,Don't Delete flowing text!
//Button NIMI // Generator NIMI 
//Button NIMI 100 // Generator NIMI and Delay 100ms, 100 not is nessary
//Button INT0 // Generator INT0 and Delay 200ms
//Button RESETAMBE3000
//Button RESET3252
//Send 1 command, Receive 2 response with one is not verify.
//Command ID: CARRIER_LOST // necessary!
//Summary  // not essential, 
//Send command: 61 00 02 00 19 00 // necessary!
//Pause=300 // not essential, unit: ms; Pause 300ms after Send command
//Timeout=100 // not essential, unit: ms; if not receive '84 A9 61 ...' in 100ms after send command, Timeout error will happen!
//*Receive Data: 61 00 02 51 19 00 // not essential, receive but not verify
//Receive Data: 61 00 02 51 19 20 // not essential, receive and verify 
//.Set x = AA B0  -- Define var x ; Added in ver2.2
// ... 61 00 02 00 19 {x}   --- use the defined var, The {x} will be replaced with AA B0 
//

.Set READY_VAR = 01
Command ID: PROCESS_MODE
Send command: 84 A9 61 00 02 00 1A 83
Receive Data: 84 A9 61 00 02 00 1A 00
Command ID:	PROTOCOL_OPTION  
Send	Command: 84 A9 61 00 02 00 55 80
Receive	Data:84 A9 61 00 02 00 55 00
Command ID: DPMR_CCH_UE_0
Send command: 84 A9 61 00 08 03 44 00 ff 22 33 44 55 FF
Receive Data: 84 A9 61 00 02 03 44 00
Command ID: DPMR_CCH_UE_1
Send command: 84 A9 61 00 08 03 44 01 ff 22 33 44 55 FF
Receive Data: 84 A9 61 00 02 03 44 00
Command ID: DPMR_CCH_UE_2
Send command: 84 A9 61 00 08 03 44 02 ff 22 33 44 55 FF
Receive Data: 84 A9 61 00 02 03 44 00
Command ID: DPMR_CCH_UE_3
Send command: 84 A9 61 00 08 03 44 03 ff 22 33 44 55 FF
Receive Data: 84 A9 61 00 02 03 44 00
Command ID: DPMR_HI_UE
Send command: 84 A9 61 00 0A 03 49 09 88 77 66 55 44 30 22 11
Receive Data: 84 A9 61 00 02 03 49 00
Command ID: DPMR_END_UE
Send command: 84 A9 61 00 04 03 4B 33 44 FF
Receive Data: 84 A9 61 00 02 03 4B 00
Command ID: REPORT_FIELD
Send command: 84 A9 61 00 02 00 1D 70
Receive Data: 84 A9 61 00 02 00 1D 00
Command ID: WORK_MODE_DUPLEX
Send command: 84 A9 61 00 04 00 18 03 00 00
Receive Data: 84 A9 61 00 02 00 18 00
Command ID: SEND_END_CLOST
Send command: 84 A9 61 00 03 00 61 19 00
Receive Data: 84 A9 61 00 02 00 19 00
Receive Data: 84 A9 61 00 02 20 17 0A
PAUSE 1000
Command ID: SEND_HEAD_SF_CREADY
Send command: 84 A9 61 00 04 00 60 5F 19 {READY_VAR}
Receive Data: 84 A9 61 00 02 00 19 00
Receive	Data:84 A9 61 00 02 30 1B 09
Receive Data: 84 A9 61 00 03 30 57 04 22
Receive Data: 84 A9 61 00 02 30 54 02
Receive Data: 84 A9 61 00 04 30 50 98 87 76
Receive	Data:84 A9 61 00 02 30 27 05
PAUSE 500
Command ID: READ_DPMR_CCH_UE
Send command: 84 A9 61 00 02 23 44 00
Receive Data: 84 A9 61 00 08 23 44 00 3f 22 33 44 55 FF
Command ID: READ_DPMR_CCH_UE
Send command: 84 A9 61 00 02 23 44 01
Receive Data: 84 A9 61 00 08 23 44 01 7f 22 33 44 55 FF
Command ID: READ_DPMR_CCH_UE
Send command: 84 A9 61 00 02 23 44 02
Receive Data: 84 A9 61 00 08 23 44 02 bf 22 33 44 55 FF
Command ID: READ_DPMR_CCH_UE
Send command: 84 A9 61 00 02 23 44 03
Receive Data: 84 A9 61 00 08 23 44 03 ff 22 33 44 55 FF
Command ID: RFAR_DPMR_CCH_UE
Send command: 84 A9 61 00 02 33 44 00
Receive Data: 84 A9 61 00 08 33 44 00 3f 22 33 44 55 80
Command ID: RFAR_DPMR_CCH_UE
Send command: 84 A9 61 00 02 33 44 01
Receive Data: 84 A9 61 00 08 33 44 01 7f 22 33 44 55 80
Command ID: RFAR_DPMR_CCH_UE
Send command: 84 A9 61 00 02 33 44 02
Receive Data: 84 A9 61 00 08 33 44 02 bf 22 33 44 55 80
Command ID: RFAR_DPMR_CCH_UE
Send command: 84 A9 61 00 02 33 44 03
Receive Data: 84 A9 61 00 08 33 44 03 ff 22 33 44 55 80
Command ID: READ_DPMR_HI_UE
Send command: 84 A9 61 00 01 23 49
Receive Data: 84 A9 61 00 0A 23 49 09 88 77 66 55 44 30 22 11
Command ID: RFAR_DPMR_HI_UE
Send command: 84 A9 61 00 01 33 49
Receive Data: 84 A9 61 00 0A 33 49 09 88 77 66 55 44 30 22 11
Command ID: REPORT_FIELD
Send command: 84 A9 61 00 02 00 1D 70
Receive Data: 84 A9 61 00 02 00 1D 00
Command ID: DPMR_SEND_END
Send command: 84 A9 61 00 01 03 61
Receive Data: 84 A9 61 00 02 03 61 00
Receive Data: 84 A9 61 00 02 20 17 0A
Receive Data: 84 A9 61 00 04 30 4B 33 44 80
PAUSE 500
Command ID: READ_DPMR_END_UE
Send command: 84 A9 61 00 01 23 4B
Receive Data: 84 A9 61 00 04 23 4B 33 44 FF
Command ID: RFAR_DPMR_END_UE
Send command: 84 A9 61 00 01 33 4B
Receive Data: 84 A9 61 00 04 33 4B 33 44 80
Command ID: CARRIER_LOST
Send command: 84 A9 61 00 02 00 19 00
Receive Data: 84 A9 61 00 02 00 19 00
PAUSE 500
Command ID: PROCESS_MODE
Send command: 84 A9 61 00 02 00 1A 02
Receive Data: 84 A9 61 00 02 00 1A 00
Command ID: SEND_HEAD_SF_CREADY
Send command: 84 A9 61 00 04 00 60 5F 19 {READY_VAR}
Receive Data: 84 A9 61 00 02 00 19 00
Receive Data: 84 A9 61 00 03 30 57 04 22
Receive Data: 84 A9 61 00 02 30 54 02
Receive Data: 84 A9 61 00 04 30 50 98 87 76
PAUSE 500
Command ID: DPMR_M_F
Send command: 84 A9 61 00 02 03 54 FF
Receive Data: 84 A9 61 00 02 03 54 00
Command ID: DPMR_END_UE
Send command: 84 A9 61 00 04 03 4B 1F 28 00
Receive Data: 84 A9 61 00 02 03 4B 00
PAUSE 500
Command ID: READ_DPMR_M_F
Send command: 84 A9 61 00 01 23 54
Receive Data: 84 A9 61 00 02 23 54 FF
Command ID: RFAR_DPMR_M_F
Send command: 84 A9 61 00 01 33 54
Receive Data: 84 A9 61 00 02 33 54 FF
Command ID: READ_DPMR_SLD
Send command: 84 A9 61 00 01 23 56
Receive Data: 84 A9 61 00 04 23 56 A2 2A C0
Command ID: RFAR_DPMR_SLD
Send command: 84 A9 61 00 01 33 56
Receive Data: 84 A9 61 00 04 33 56 A2 2A C0
Command ID: DPMR_SEND_END
Send command: 84 A9 61 00 01 03 61
Receive Data: 84 A9 61 00 02 03 61 00
Receive Data: 84 A9 61 00 02 20 17 0A
Receive Data: 84 A9 61 00 04 30 4B 1F 28 00
PAUSE 500
Command ID: READ_DPMR_END_UE
Send command: 84 A9 61 00 01 23 4B
Receive Data: 84 A9 61 00 04 23 4B 1F 28 00
Command ID: RFAR_DPMR_END_UE
Send command: 84 A9 61 00 01 33 4B
Receive Data: 84 A9 61 00 04 33 4B 1F 28 00
Command ID: CARRIER_LOST
Send command: 84 A9 61 00 02 00 19 00
Receive Data: 84 A9 61 00 02 00 19 00
Command ID: AMLOOP_CODEC_CODEC_LOOP
Send command: 84 A9 61 00 04 00 18 03 11 00
Receive Data: 84 A9 61 00 02 00 18 00
