//Verison=2.2
//Example,Don't Delete flowing text!
//Button NIMI // Generator NIMI 
//Button NIMI 100 // Generator NIMI and Delay 100ms, 100 not is nessary
//Button INT0 // Generator INT0 and Delay 200ms
//Button RESETAMBE3000
//Button RESET3252
//Send 1 command, Receive 2 response with one is not verify.
//Command ID: CARRIER_LOST // necessary!
//Summary  // not essential, 
//Send command: 61 00 02 00 19 00 // necessary!
//Pause=300 // not essential, unit: ms; Pause 300ms after Send command
//Timeout=100 // not essential, unit: ms; if not receive '84 A9 61 ...' in 100ms after send command, Timeout error will happen!
//*Receive Data: 61 00 02 51 19 00 // not essential, receive but not verify
//Receive Data: 61 00 02 51 19 20 // not essential, receive and verify 
//.Set x = AA B0  -- Define var x ; Added in ver2.2
// ... 61 00 02 00 19 {x}   --- use the defined var, The {x} will be replaced with AA B0 
//
.Set x = FF BF 
.Set y = 17 04
.set z = 17 06

Command ID:	VOCODER_SEL
Send	Command: 84 A9 61 00 02 00 10 13
Receive	Data:84 A9 61 00 02 00 10 00
pause 3000
Command ID:	VOCODER_SEL
Send	Command: 84 A9 61 00 02 00 10 03
Receive	Data:84 A9 61 00 02 00 10 00
pause 2000
Command ID:   DPMR_CCH_CCH_UE_0
Send command: 84 A9 61 00 08 03 44 00 00 22 33 44 55 FF
Receive Data: 84 A9 61 00 02 03 44 00
Command ID:   DPMR_CCH_UE_1
Send command: 84 A9 61 00 08 03 44 01 11 22 33 44 55 FF
Receive Data: 84 A9 61 00 02 03 44 00
Command ID:   DPMR_CCH_UE_2
Send command: 84 A9 61 00 08 03 44 02 22 22 33 44 55 FF
Receive Data: 84 A9 61 00 02 03 44 00
Command ID:   DPMR_CCH_UE_3
Send command: 84 A9 61 00 08 03 44 03 33 22 33 44 55 FF
Receive Data: 84 A9 61 00 02 03 44 00
Command ID:   READ_DPMR_CCH_UE
Send command: 84 A9 61 00 02 23 44 00
Receive Data: 84 A9 61 00 08 23 44 00 00 22 33 44 55 FF
Command ID:   READ_DPMR_CCH_UE
Send command: 84 A9 61 00 02 23 44 01
Receive Data: 84 A9 61 00 08 23 44 01 51 22 33 44 55 FF
Command ID:   READ_DPMR_CCH_UE
Send command: 84 A9 61 00 02 23 44 02
Receive Data: 84 A9 61 00 08 23 44 02 A2 22 33 44 55 FF
Command ID:   READ_DPMR_CCH_UE
Send command: 84 A9 61 00 02 23 44 03
Receive Data: 84 A9 61 00 08 23 44 03 F3 22 33 44 55 FF
Command ID:   READ_DPMR_CCH_UE
Send command: 84 A9 61 00 02 23 44 00
Receive Data: 84 A9 61 00 08 23 44 00 00 22 33 44 55 FF
Command ID:   RFAR_DPMR_CCH_UE
Send command: 84 A9 61 00 02 33 44 00
Receive Data: 84 A9 61 00 08 33 44 00 00 00 00 00 00 00
Command ID:   RFAR_DPMR_CCH_UE
Send command: 84 A9 61 00 02 33 44 01
Receive Data: 84 A9 61 00 08 33 44 01 00 00 00 00 00 00
Command ID:   RFAR_DPMR_CCH_UE
Send command: 84 A9 61 00 02 33 44 02
Receive Data: 84 A9 61 00 08 33 44 02 00 00 00 00 00 00
Command ID:   RFAR_DPMR_CCH_UE
Send command: 84 A9 61 00 02 33 44 03
Receive Data: 84 A9 61 00 08 33 44 03 00 00 00 00 00 00
Command ID:   RFAR_DPMR_CCH_UE
Send command: 84 A9 61 00 02 33 44 00
Receive Data: 84 A9 61 00 08 33 44 00 00 00 00 00 00 00	
Command ID:   DPMR_CCH_UE1                                                                                         
Send command: 84 A9 61 00 07 00 44 00 00 22 33 44 55 FF                                                            
Receive Data: 84 A9 61 00 02 00 {z}                                                                              
Command ID:   DPMR_CCH_UE2                                                                                         
Send command: 84 A9 61 00 09 00 44 00 00 22 33 44 55 FF {x}                                                        
Receive Data: 84 A9 61 00 02 00 17 04                                                                              
Command ID:   DPMR_CCH_UE3                                                                                         
Send command: 84 A9 61 00 02 20 44                                                                                 
Receive Data: 84 A9 61 00 08 20 44 00 00 22 33 44 55 FF                                                      
Command ID:   DPMR_HI_UE1                                                                                          
Send command: 84 A9 61 00 09 00 49 09 88 77 66 55 44 30 22 11                                                      
Receive Data: 84 A9 61 00 02 00 {z}                                                                              
Command ID:   DPMR_HI_UE2                                                                                          
Send command: 84 A9 61 00 0C 00 49 09 88 77 66 55 44 30 22 11 {x}                                                  
Receive Data: 84 A9 61 00 02 00 17 04                                                                              
Command ID:   DPMR_HI_UE3                                                                                          
Send command: 84 A9 61 00 01 20 49                                                                                 
Receive Data: 84 A9 61 00 0A 20 49 09 88 77 66 55 44 30 22 11                                                      
                                                                                                                   
