This program is an example of the startup sequence for HackRF (Jellybean with
Lemondrop attached).
LED1, LED2, and LED3 are blinking at exactly a frequency of 1Hz upon success.

Required Lemondrop -> Jellybean connections:

SCL: Lemondrop P7 pin 3 -> Jellybean P6 pin 3
SDA: Lemondrop P7 pin 5 -> Jellybean P6 pin 5
SDA: Lemondrop P7 pin 6 -> Jellybean P6 pin 6
VCC: Lemondrop P4 pin 2, 4, or 6 -> Jellybean P17 pin 2, 4, or 6
1V8: Lemondrop P11 pin 2, 4, or 6 -> Jellybean P16 pin 2, 4, or 6
GND: Lemondrop P5 -> Jellybean P13
